Delay:

NSC HYPERchannel-D X within NCET4 card

0

1

2

3

4

5

64 512 1024 Packet Length

Delay msec