Delay:

Wellfleet - within interface board

0

1

2

3

4

5

64 512 1024 Packet Length

Delay msec